고가 분취컬럼 필요없는 한번에 98%이상 회수율의 고성능 원심분배 크로마토그라프(HPCPC) 의 기작 이해

An innovative liquid-liquid chromatography without solid support

Centrifugal Partition Chromatography (CPC) is a separation method based on the liquid partition of compounds. Due to the centrifugal field force, one phase stays in the rotor (the stationnary phase), the other one is the mobile as in classical chromatography. The compounds migrate through the rotor according to their partition coefficient Kd:

Process for the separation of three compounds with different partition coefficient:

High Performance Centrifugal Partition Chromatograph

고속의 용매 전달 장치를 이용하여 짧은 시간에 많은 양의 혼합시료를 이동상 과 함께 고속회전 원심력 액체 분리 디스크채널내의 고정상을 통하여 흐르게 하여 고정상과 이동상에 대한 각 시료성분의 물리화학적 성질의 차이에 의해 분리한 다음, 적합한 분취기를 이용하여 원하는 물질을 분취한다. 일반 분석용 HPLC와 달리 대용량 시료 주입기, 대용량 펌프, 대용량 UV/VIS 검출기등이 분리에 사용된다.

이에 대용량 유체 시료 전달장치와 대용량 원심력 회전 원통방식 디스크채 널분리관이 반드시 필요 하다.

Extraction and Purification of all types of Molecules from Natural and Synthetic Extracts

HPCPC has a wide range of applications. All organic and inorganic molecules can be processed. These are usually classified from the polar to non polar.

Selection of Two-Phase Partition Solvents

A two-phase solvent system is used as separation medium in Centrifugal Partition Chromatography. One serves as the stationary phase, the other serves as the mobile phase. The solvents may be selected from an infinite variety of possible combinations. Followings are some frequently used solvent combinations.